{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["QUARTERLY","FALL","SPRING"],"not_rendered":{"images":2},"read":"whole","date_system":"1900"}

{"sheet":"QUARTERLY","index":0,"n_rows":10,"n_cols":7,"rows_kept":10,"merged":[[3,4,3,6]]}
[]
[null,"HOME MAINTENANCE SCHEDULE"]
[]
[null,"QUARTERLY",null,null,"DATE LAST COMPLETED"]
[null,"CATEGORY","ACTIVITY","DESCRIPTION","DATE 1","DATE 2","DATE 3"]
[null,"Plumbing","Faucets and shower heads","Check interior and exterior faucets for leaks. Clean aerators. Replace washers if necessary."]
[null,"Interior","Wood cabinets and trim","Apply a wood protectant."]
[null,"Electrical and Appliances","GFI outlets","Test for proper operation."]
[null,"Exterior","Landscaping","Check for proper drainage. "]
[null,"Interior","Interior doors","Lubricate hinges."]

{"sheet":"FALL","index":1,"n_rows":9,"n_cols":7,"rows_kept":9,"merged":[[1,4,1,6]]}
[]
[null,"FALL",null,null,"DATE LAST COMPLETED"]
[]
[null,"CATEGORY","ACTIVITY","DESCRIPTION","DATE 1","DATE 2","DATE 3"]
[null,"Plumbing","Plumbing shut-off valves","Inspect for proper operation."]
[null,"Interior","Countertops","Inspect for separations at sinks and backsplash. Recaulk where required."]
[null,"Electrical and Appliances","Heating system","Service heating system and heat pump."]
[null,"Exterior","Roof","Check for leaks. Check for damaged, loose, or missing shingles. Check vents and louvers for birds, nests, squirrels, and insects. Check flashing around roof stacks, vents, and skylights for leaks."]
[null,"Interior","Countertops","Inspect for separations at sinks and backsplash. Recaulk where required."]

{"sheet":"SPRING","index":2,"n_rows":9,"n_cols":7,"rows_kept":9,"merged":[[1,4,1,6]]}
[]
[null,"SPRING",null,null,"DATE LAST COMPLETED"]
[]
[null,"CATEGORY","ACTIVITY","DESCRIPTION","DATE 1","DATE 2","DATE 3"]
[null,"Interior","Attic","Examine for evidence of any leaks. Check insulation and remove or add if necessary. Check for evidence of birds, squirrels, raccoons, etc. Check for proper ventilation."]
[null,"Plumbing","Water heater","Flush out hot water to remove accumulated sediment."]
[null,"Electrical and Appliances","Heating and cooling system","General furnace inspection: Look for rust, scaling on heat exchanger, and proper flame color; note odd sounds or smells; and check condition of venting. Remove debris around units."]
[null,"Interior","Shower doors/tub enclosures","Inspect for proper fit. Adjust if necessary. Inspect caulking and recaulk if necessary."]
[null,"Exterior","Decks","Scrub mildewed areas and treat for water stains, mildew, and fungus."]