{"text_format":"1","workbook":"xls","n_sheets":1,"sheets":["Home Maintenance Schedule"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Home Maintenance Schedule","index":0,"n_rows":79,"n_cols":3,"rows_kept":79,"cut":false,"hidden":false,"merged":[[2,2,2,5],[29,2,29,5],[57,2,57,5],[0,2,0,5]],"flags":["formulas_cached_only"]}
["Home Maintenance Schedule",null,"This is a starting list; you may want to add or remove items by inserting and deleting rows on this worksheet."]
[]
["Quarterly",null,"Date last completed"]
["Plumbing"]
["Faucets and shower heads","Check interior and exterior faucets for leaks. Clean aerators. Replace washers if necessary."]
["Drains","Clean with baking soda. Pour water down unused drains."]
["Pipes","Inspect visible pipes for leaks."]
["Kitchen and bathroom cabinets","Check under and around for leaks."]
["Toilets","Check for stability and leaks."]
["Water heater","Check area around water heater for leaks. If you have hard water, drain 1-2 gallons water."]
["Interior"]
["Wood cabinets and trim","Apply a wood protectant."]
["Interior doors","Lubricate hinges."]
["Garage door","Lubricate hardware. Inspect mechanism for free travel."]
["Window and door tracks","Check to see if weep holes are open. Clean out dirt and dust. Lubricate rollers and latches."]
["Basement or crawl space","Check for cracks or any sign of dampness or leaks. Check for any evidence of termites or wood-eating insects."]
["Ceramic tile","Check and clean grout."]
["Electrical and appliances"]
["Heating and cooling systems","Clean and replace filters if necessary."]
["Kitchen exhaust fan","Remove and clean the filter. Clean accumulated grease deposits from the fan housing."]
["Refrigerator","Clean dust from top. Clean refrigerator drain pan. Clean and defrost freezer if necessary."]
["Dishwasher","Check for leaks."]
["Wiring, electrical cords, and plugs","Check for wear or damage. Replace if necessary."]
["Smoke detector","Test for proper operation and replace batteries if necessary."]
["GFI outlets","Test for proper operation."]
["Exterior"]
["Foundation","Inspect visible areas, vents, and ducts for cracks, leaks, or blockages."]
["Landscaping","Check for proper drainage. "]
["Concrete and asphalt","Clean oil and grease."]
["Fall",null,"Date last completed"]
["Plumbing"]
["Plumbing shut-off valves","Inspect for proper operation."]
["Outside faucets","Drain."]
["Water heater","Flush out hot water to remove accumulated sediment."]
["Faucet aerators","Check for proper flow of water. If the flow is reduced, clean the aerator screens. During the first two months, the faucet aerators could require more frequent cleaning."]
["Interior"]
["Attic","Examine for evidence of any leaks. Check insulation and remove or add if necessary. Check for evidence of birds, squirrels, raccoons, etc. Check for proper ventilation."]
["Countertops","Inspect for separations at sinks and backsplash. Recaulk where required."]
["Tiled areas","Inspect for loose or missing grout or caulking. Regrout or recaulk if necessary."]
["Shower doors/tub enclosures","Inspect for proper fit. Adjust if necessary. Inspect caulking and recaulk if necessary."]
["Weather stripping","Check caulking around windows and doors. Check window and door screens. Adjust or replace if necessary."]
["Sectional garage doors","Adjust the travel and tension."]
["Fireplace","Inspect flues. Clean if necessary. Inspect fireplace brick and mortar for cracks or damage. "]
["Electrical and appliances"]
["Heating system","Service heating system and heat pump."]
["Cooling system","Remove debris from around units and clean with garden hose. Remove window air conditioner or protect with weatherproof cover. Clean and replace filters if necessary."]
["Refrigerator coils","Clean."]
["Combustible appliances","Inspect and service if necessary."]
["Exterior"]
["Roof","Check for leaks. Check for damaged, loose, or missing shingles. Check vents and louvers for birds, nests, squirrels, and insects. Check flashing around roof stacks, vents, and skylights for leaks."]
["Chimney","Clean and check for deteriorating bricks and mortar. Check for leaks. Check for birds, nests, squirrels, and insects."]
["Gutters and downspouts","Clean and check for leaks, misalignment, or damage."]
["Exterior walls","Check for deteriorating bricks and mortar. Check siding for damage or rot. Check painted surfaces for flaking."]
["Landscaping","Trim shrubbery around walls. Remove tree limbs, branches, or debris that can attract insects (no wood or shrubbery should be closer than 3 inches to your house). Maintain grading."]
["Concrete and asphalt","Check for cracks or deterioration. Reseal or repair if necessary."]
["Septic system","Examine septic system drain field for flooding and odor. Have tank pumped yearly."]
["Lawn and patio furniture","Clean and store or cover with weatherproof material."]
["Spring",null,"Date last completed"]
["Plumbing"]
["Water heater","Flush out hot water to remove accumulated sediment."]
["Interior"]
["Attic","Examine for evidence of any leaks. Check insulation and remove or add if necessary. Check for evidence of birds, squirrels, raccoons, etc. Check for proper ventilation."]
["Countertops","Inspect for separations at sinks and backsplash. Recaulk where required."]
["Tiled areas","Inspect for loose or missing grout or caulking. Regrout or recaulk if necessary."]
["Shower doors/tub enclosures","Inspect for proper fit. Adjust if necessary. Inspect caulking and recaulk if necessary."]
["Weather stripping","Check caulking around windows and doors. Check window and door screens. Adjust or replace if necessary."]
["Electrical and appliances"]
["Heating and cooling system","General furnace inspection: Look for rust, scaling on heat exchanger, and proper flame color; note odd sounds or smells; and check condition of venting. Remove debris around units."]
["Circuit breakers ","Exercise."]
["Refrigerator","Clean coils."]
["Exterior"]
["Decks","Scrub mildewed areas and treat for water stains, mildew, and fungus."]
["Roof","Clean. Check for leaks. Check for damaged, loose or missing shingles. Check vents and louvers for birds, nests, squirrels, and insects. Check flashing around roof stacks, vents, and skylights for leaks."]
["Chimney","Clean and check for deteriorating bricks and mortar. Check for leaks. Check for birds, nests, squirrels, and insects."]
["Gutters and downspouts","Clean and check for leaks, misalignment, or damage."]
["Windows","Clean."]
["Exterior walls","Check for deteriorating bricks and mortar. Check siding for damage or rot. Check painted surfaces for flaking."]
["Landscaping","Trim shrubbery around walls. Remove tree limbs, branches, or debris that can attract insects (no wood or shrubbery should be closer than 3 inches to your house). Maintain grading."]
["Concrete and asphalt","Check for cracks or deterioration. Reseal or repair if necessary."]