{"text_format":"1","workbook":"xls","n_sheets":1,"sheets":["房屋维护计划"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"房屋维护计划","index":0,"n_rows":79,"n_cols":3,"rows_kept":79,"cut":false,"hidden":false,"merged":[[57,2,57,5],[0,0,0,5],[1,0,1,2],[2,2,2,5],[29,2,29,5]],"flags":["formulas_cached_only"]}
["房屋维护计划"]
["这是原始列表，您可以通过在工作表中添加或删除行来添加或删除条目。"]
["每季度的维护项目",null,"最终完成日期"]
["水暖管件"]
["水龙头和淋浴龙头","检查内部和外部水龙头是否渗漏。清理通风装置。必要时更换垫圈。"]
["排水管","用苏打水进行清理。注水冲洗未用过的排水管。"]
["管道","查看裸露的管道是否渗漏。"]
["厨房和浴室柜","仔细查看是否渗漏。"]
["马桶","检查马桶的使用是否正常，是否有渗漏。"]
["热水器","查看热水器周围是否渗漏。如果有硬水，排干 1-2 公升水。"]
["内部"]
["木制厨柜和装修","使用木材保护剂。"]
["室内门","润滑门合页。"]
["车库门","润滑五金件。检查自由通行装置。"]
["窗户和门导轨","检查泄水孔是否堵塞。清理其中的脏物。润滑滚轴和插销。"]
["地下室或线槽","查看是否有裂纹或任何潮湿或渗透的痕迹。查看是否有白蚁或蛀虫活动的痕迹。"]
["瓷砖","检查并清理泥浆。"]
["电器"]
["供暖和制冷系统","如果必要，清理并更换过滤器。"]
["厨房排气风扇","拆洗过滤器。清理风扇罩中积聚的油污。"]
["电冰箱","清理灰尘。清理冰箱排水盘。如必要，解冻并清理冷冻室。"]
["洗碗机","检查是否渗漏。"]
["接线和插头","检查是否磨损和损坏。必要时更换。"]
["烟雾探测器","检查工作是否正常，必要时更换电池。"]
["GFI 插座","检查工作是否正常。"]
["外部"]
["基础设施","检查可见区域、通风孔，并检查管道是否有裂缝、泄漏或堵塞。"]
["景观设施","检查排水装置。 "]
["混凝土和沥青","清除油脂。"]
["秋季维护项目",null,"最终完成日期"]
["水暖管件"]
["水管阀门","检查工作是否正常。"]
["户外水龙头","排水。"]
["热水器","用热水冲洗积聚的水垢。"]
["水龙头空气混合阀","检查水流。如果水流变小，清理空气混合阀网。在头两个月里，水龙头空气混合阀需要经常清洗。"]
["内部"]
["阁楼","检查所有渗漏的痕迹。检查绝缘设施，必要时进行拆除和增设。检查是否有鸟类、松鼠等动物痕迹。检查通风情况。"]
["厨房操作台","检查水槽和后防溅板的分隔区。必要时重新填充以防渗漏。"]
["瓦面排水区","检查砂浆或填充物是否有松动或缺损。必要时重新涂抹砂浆或重新填充。"]
["淋浴房门/浴缸防漏","检查安装是否合适，必要时进行调整。检查填缝情况，必要时重新填缝。"]
["挡风雨条","检查窗户和门周围的缝条。检查窗纱和门纱。"]
["组合式车库门","调整行程和拉力。"]
["壁炉","检查烟道。必要时进行清理。检查壁炉砖和墙面是否有裂逢或破损。"]
["电器"]
["供暖系统","维修供暖系统和加热泵。"]
["制冷系统","清除装置周围的碎屑，并用橡胶软管进行清理。拆卸窗式空调并用防雨罩进行保护。如果必要，清理并更换过滤器。"]
["冰箱线圈","清理。"]
["易燃器具","如必要，进行检查和维修。"]
["外部"]
["屋顶","检查渗漏。检查屋顶板是否有损坏、松动或缺损。检查通风口和天窗，查看是否存在鸟类、鸟巢、松鼠和昆虫。检查屋顶、通风口和天窗周围的防水板是否渗漏。"]
["烟囱","清理并检查是否存在损坏的砖块和水泥。检查渗漏。检查是否存在鸟类、鸟巢、松鼠和昆虫。"]
["水槽和下水管","清理并检查是否有渗漏、安装不准确或损坏。"]
["外墙","检查是否有损坏的砖块和水泥。检查壁板是否有损坏或腐烂。检查油漆是否脱落。"]
["景观设施","修整围墙四周的灌木丛。修剪树枝，除去那些容易招昆虫的碎屑（房子 3 英寸以内不应存在树木或灌木）。维修路基。"]
["混凝土和沥青","检查是否有裂缝或磨损。必要时重新填封或修补。"]
["化粪系统","检查化粪系统排污管道是否有溢出现象和发出气味。每年清理一次化粪池。"]
["草坪和院子里的家具","清理并储存，或用防雨材料遮盖。"]
["春季维护项目",null,"最终完成日期"]
["水管装置"]
["热水器","用热水冲洗积聚的水垢。"]
["内部"]
["阁楼","检查所有渗漏痕迹。检查绝缘设施，必要时进行拆除和增设。检查是否有鸟类、松鼠、浣熊等动物痕迹。检查通风情况。"]
["厨房操作台","检查水槽和后防溅板的分隔区。必要时重新填充以防渗漏。"]
["瓦面排水区","检查砂浆或填充物是否松动或缺损。必要时重新涂抹砂浆或重新填充。"]
["淋浴房门/浴缸防漏","检查是否合适。必要时进行调整。必要时检查填缝情况或重新填缝。"]
["挡风雨条","检查窗户和门周围的填缝。检查窗纱和门纱。"]
["电器"]
["供暖和制冷系统","检查加热炉：查看是否有铁锈、调节旋扭工作是否正常、以及火焰颜色是否正常；注意声音或气味是否异常；查看通风状况。清除装置中的碎屑。"]
["断路开关 ","测试。"]
["电冰箱","清理线圈。"]
["外部"]
["露台","擦洗霉斑，并清除水渍、霉菌等。"]
["屋顶","进行清理。检查渗漏。检查屋顶是否有损坏、松动或缺损。检查通风口和天窗，查看是否存在鸟类、鸟巢、松鼠和昆虫。检查屋顶、通风口和天窗周围的防水板是否渗漏。"]
["烟囱","清理并检查是否存在损坏的砖块和水泥。检查渗漏。检查是否存在鸟类、鸟巢、松鼠和昆虫。"]
["水槽和下水管","清理并检查是否有渗漏、安装不准确或损坏等。"]
["窗户","清理。"]
["外墙","检查是否有损坏的砖块和水泥。检查壁板是否有损坏或腐烂。检查油漆是否脱落。"]
["景观设施","修整围墙四周的灌木丛。修剪树枝、或清除那些容易招昆虫的碎屑（房子 3 英寸以内不应存在树木或灌木）。维修路基。"]
["混凝土和沥青","检查是否有裂缝或磨损。必要时重新填封或修补。"]