{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["QUARTERLY","AUTUMN","SPRING"],"not_rendered":{"defined_names":3},"read":"whole","date_system":"1900"}

{"sheet":"QUARTERLY","index":0,"n_rows":8,"n_cols":7,"rows_kept":8,"merged":[[0,1,0,6],[1,1,1,3],[1,4,1,6]]}
[null,"HOME MAINTENANCE SCHEDULE"]
[null,"QUARTERLY",null,null,"Date last completed"]
[null,"Category","Activity","Description","Date 1","Date 2","Date 3"]
[null,"Plumbing","Taps and shower heads","Check interior and exterior taps for leaks. Clean aerators. Replace washers if necessary."]
[null,"Interior","Wooden cabinets and trim","Apply a wood protectant."]
[null,"Electrical and Appliances","GFI outlets","Test for proper operation."]
[null,"Exterior","Landscaping","Check for proper drainage. "]
[null,"Interior","Interior doors","Lubricate hinges."]

{"sheet":"AUTUMN","index":1,"n_rows":7,"n_cols":7,"rows_kept":7,"merged":[[0,1,0,3],[0,4,0,6]]}
[null,"AUTUMN",null,null,"Date last completed"]
[null,"Category","Activity","Description","Date 1","Date 2","Date 3"]
[null,"Plumbing","Plumbing shut-off valves","Inspect for proper operation."]
[null,"Interior","Worktops","Inspect for separations at sinks and backsplash. Recaulk where required."]
[null,"Electrical and Appliances","Heating system","Service heating system and heat pump."]
[null,"Exterior","Roof","Check for leaks. Check for damaged, loose or missing shingles. Check vents and louvres for birds, nests, squirrels and insects. Check flashing around roof stacks, vents and skylights for leaks."]
[null,"Interior","Worktops","Inspect for separations at sinks and backsplash. Recaulk where required."]

{"sheet":"SPRING","index":2,"n_rows":7,"n_cols":7,"rows_kept":7,"merged":[[0,1,0,3],[0,4,0,6]]}
[null,"SPRING",null,null,"Date last completed"]
[null,"Category","Activity","Description","Date 1","Date 2","Date 3"]
[null,"Interior","Attic","Examine for evidence of any leaks. Check insulation and remove or add if necessary. Check for evidence of birds, squirrels, bats etc. Check for proper ventilation."]
[null,"Plumbing","Water heater","Flush out hot water to remove accumulated sediment."]
[null,"Electrical and Appliances","Heating and cooling system","General furnace inspection: Look for rust, scaling on heat exchanger and proper flame colour; note odd sounds or smells; and check condition of venting. Remove debris around units."]
[null,"Interior","Shower doors/bathtub enclosures","Inspect for proper fit. Adjust if necessary. Inspect caulking and recaulk if necessary."]
[null,"Exterior","Decks","Scrub mildewed areas and treat for water stains, mildew and fungus."]